# Configure MiVoice Business for BLF

To set up BLF for the MiVoice Business Console, you must program some options in ESM on the MiVoice Business.

1. Connect to ESM by clicking on Console File Menu -> Connect to ESM.

2. Select the Multiline Set Key Assignment form.

3. Select the Directory number.

4. Program the corresponding Programmable keys.

5. Change the Line Type to DSS/Busy Lamp and Ring Type to No Ring.

Parent topic: Busy Lamp Field
↑