# Options (Queued Calls)

Use this dialog box to select the incoming calls threshold and various timeout values for incoming, transferred, and parked calls.

To open this dialog

1. Select Options from the Tools menu.

2. Click the Queued Calls option.

## Incoming Calls Threshold

To reduce call-waiting times, your system may be programmed to present incoming calls to other consoles or answering positions. If your system is programmed this way, enter the number of calls that must be incoming before the system presents them to your console.

## Incoming Calls

Displays the Timeout Value for Incoming Calls, indicating the amount of time an incoming call can remain queued before a visual alert appears. Set the value in seconds from 0 to 999. The default setting is 30 seconds.

## Transferred Calls

Displays the Timeout Value for Transferred Calls, indicating the amount of time a transferred call can remain queued before a visual alert appears. Set the value in seconds from 0 to 999. The default setting in 60 seconds.

## Parked Calls

Displays the Timeout Value for Parked Calls, indicating the amount of time a parked call can remain queued before a visual alert appears. Set the value in seconds from 0 to 999. The default setting is 120 seconds.

Parent topic: Configuration Settings
↑